(kicad_pcb (version 4) (host pcbnew 4.0.3-stable)

  (general
    (links 42)
    (no_connects 42)
    (area 0 0 0 0)
    (thickness 1.6)
    (drawings 0)
    (tracks 0)
    (zones 0)
    (modules 19)
    (nets 18)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 /V_BAT)
  (net 2 GND)
  (net 3 VCC)
  (net 4 "Net-(D1-Pad2)")
  (net 5 "Net-(D2-Pad2)")
  (net 6 "Net-(D3-Pad2)")
  (net 7 "Net-(D4-Pad2)")
  (net 8 "Net-(D4-Pad1)")
  (net 9 "Net-(IC1-Pad7)")
  (net 10 "Net-(IC1-Pad6)")
  (net 11 "Net-(IC1-Pad5)")
  (net 12 "Net-(IC1-Pad3)")
  (net 13 "Net-(IC1-Pad2)")
  (net 14 "Net-(IC1-Pad1)")
  (net 15 "Net-(JP2-Pad2)")
  (net 16 "Net-(P2-Pad4)")
  (net 17 "Net-(P2-Pad6)")

  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /V_BAT)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(IC1-Pad1)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad3)")
    (add_net "Net-(IC1-Pad5)")
    (add_net "Net-(IC1-Pad6)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(JP2-Pad2)")
    (add_net "Net-(P2-Pad4)")
    (add_net "Net-(P2-Pad6)")
    (add_net VCC)
  )

  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA) (tstamp 57BE9728)
    (at 185.855001 119.045)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (path /57BD6F3C)
    (attr smd)
    (fp_text reference C1 (at 0 -2.1) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1uf (at 0 2.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.8 -1) (end 1.8 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1) (end 1.8 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1) (end -1.8 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1) (end 1.8 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /V_BAT))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA) (tstamp 57BE972E)
    (at 182.548571 125.295)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (path /57BD6FAC)
    (attr smd)
    (fp_text reference C2 (at 0 -2.1) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 2.2uf (at 0 2.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.8 -1) (end 1.8 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1) (end 1.8 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1) (end -1.8 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1) (end 1.8 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_0805 (layer F.Cu) (tedit 55BDE1C2) (tstamp 57BE9734)
    (at 180.303334 118.695)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (path /57BD75CA)
    (attr smd)
    (fp_text reference D1 (at 0 -1.75) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "blue LED" (at 0 1.75) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.4 -0.3) (end -0.4 0.3) (layer F.Fab) (width 0.15))
    (fp_line (start -0.3 0) (end 0 -0.3) (layer F.Fab) (width 0.15))
    (fp_line (start 0 0.3) (end -0.3 0) (layer F.Fab) (width 0.15))
    (fp_line (start 0 -0.3) (end 0 0.3) (layer F.Fab) (width 0.15))
    (fp_line (start 1 -0.6) (end -1 -0.6) (layer F.Fab) (width 0.15))
    (fp_line (start 1 0.6) (end 1 -0.6) (layer F.Fab) (width 0.15))
    (fp_line (start -1 0.6) (end 1 0.6) (layer F.Fab) (width 0.15))
    (fp_line (start -1 -0.6) (end -1 0.6) (layer F.Fab) (width 0.15))
    (fp_line (start -1.6 0.75) (end 1.1 0.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.6 -0.75) (end 1.1 -0.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.1 0.15) (end -0.1 -0.1) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.1 -0.1) (end -0.25 0.05) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.35 -0.35) (end -0.35 0.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 0 0) (end 0.35 0) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.35 0) (end 0 -0.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 0 -0.35) (end 0 0.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 0 0.35) (end -0.35 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.9 -0.95) (end 1.9 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.9 0.95) (end -1.9 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.9 0.95) (end -1.9 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.9 -0.95) (end 1.9 -0.95) (layer F.CrtYd) (width 0.05))
    (pad 2 smd rect (at 1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:SOD-323 (layer F.Cu) (tedit 5530FC5E) (tstamp 57BE973A)
    (at 152.73762 126.455)
    (descr SOD-323)
    (tags SOD-323)
    (path /57BD74D6)
    (attr smd)
    (fp_text reference D2 (at 0 -1.85) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D_Schottky (at 0.1 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.25 0) (end 0.5 0) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.25 0) (end -0.5 0) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.25 0) (end 0.25 -0.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.25 -0.35) (end 0.25 0.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.25 0.35) (end -0.25 0) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.25 -0.35) (end -0.25 0.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.5 -0.95) (end 1.5 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.5 -0.95) (end 1.5 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.5 0.95) (end 1.5 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.5 -0.95) (end -1.5 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.1 0.8) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.3 -0.8) (end 1.1 -0.8) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.055 0) (size 0.59 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 1.055 0) (size 0.59 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (model Diodes_SMD.3dshapes/SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module LEDs:LED_0805 (layer F.Cu) (tedit 55BDE1C2) (tstamp 57BE9740)
    (at 195.653334 103.055)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (path /57BD80DC)
    (attr smd)
    (fp_text reference D3 (at 0 -1.75) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "blue LED" (at 0 1.75) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.4 -0.3) (end -0.4 0.3) (layer F.Fab) (width 0.15))
    (fp_line (start -0.3 0) (end 0 -0.3) (layer F.Fab) (width 0.15))
    (fp_line (start 0 0.3) (end -0.3 0) (layer F.Fab) (width 0.15))
    (fp_line (start 0 -0.3) (end 0 0.3) (layer F.Fab) (width 0.15))
    (fp_line (start 1 -0.6) (end -1 -0.6) (layer F.Fab) (width 0.15))
    (fp_line (start 1 0.6) (end 1 -0.6) (layer F.Fab) (width 0.15))
    (fp_line (start -1 0.6) (end 1 0.6) (layer F.Fab) (width 0.15))
    (fp_line (start -1 -0.6) (end -1 0.6) (layer F.Fab) (width 0.15))
    (fp_line (start -1.6 0.75) (end 1.1 0.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.6 -0.75) (end 1.1 -0.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.1 0.15) (end -0.1 -0.1) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.1 -0.1) (end -0.25 0.05) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.35 -0.35) (end -0.35 0.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 0 0) (end 0.35 0) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.35 0) (end 0 -0.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 0 -0.35) (end 0 0.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 0 0.35) (end -0.35 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.9 -0.95) (end 1.9 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.9 0.95) (end -1.9 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.9 0.95) (end -1.9 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.9 -0.95) (end 1.9 -0.95) (layer F.CrtYd) (width 0.05))
    (pad 2 smd rect (at 1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_0805 (layer F.Cu) (tedit 55BDE1C2) (tstamp 57BE9746)
    (at 194.348572 114.855)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (path /57BD624D)
    (attr smd)
    (fp_text reference D4 (at 0 -1.75) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "red LED" (at 0 1.75) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.4 -0.3) (end -0.4 0.3) (layer F.Fab) (width 0.15))
    (fp_line (start -0.3 0) (end 0 -0.3) (layer F.Fab) (width 0.15))
    (fp_line (start 0 0.3) (end -0.3 0) (layer F.Fab) (width 0.15))
    (fp_line (start 0 -0.3) (end 0 0.3) (layer F.Fab) (width 0.15))
    (fp_line (start 1 -0.6) (end -1 -0.6) (layer F.Fab) (width 0.15))
    (fp_line (start 1 0.6) (end 1 -0.6) (layer F.Fab) (width 0.15))
    (fp_line (start -1 0.6) (end 1 0.6) (layer F.Fab) (width 0.15))
    (fp_line (start -1 -0.6) (end -1 0.6) (layer F.Fab) (width 0.15))
    (fp_line (start -1.6 0.75) (end 1.1 0.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.6 -0.75) (end 1.1 -0.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.1 0.15) (end -0.1 -0.1) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.1 -0.1) (end -0.25 0.05) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.35 -0.35) (end -0.35 0.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 0 0) (end 0.35 0) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.35 0) (end 0 -0.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 0 -0.35) (end 0 0.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 0 0.35) (end -0.35 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.9 -0.95) (end 1.9 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.9 0.95) (end -1.9 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.9 0.95) (end -1.9 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.9 -0.95) (end 1.9 -0.95) (layer F.CrtYd) (width 0.05))
    (pad 2 smd rect (at 1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D4-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module SMD_Packages:SOIC-8-N (layer F.Cu) (tedit 0) (tstamp 57BE9752)
    (at 187.498571 104.2765)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (path /57BD5CB6)
    (attr smd)
    (fp_text reference IC1 (at 0 -1.27) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value ATTINY85-S (at 0 1.27) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.54 -2.286) (end 2.54 -2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 -2.286) (end 2.54 2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.54 2.286) (end -2.54 2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.54 2.286) (end -2.54 -2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.54 -0.762) (end -2.032 -0.762) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.032 -0.762) (end -2.032 0.508) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.032 0.508) (end -2.54 0.508) (layer F.SilkS) (width 0.15))
    (pad 8 smd rect (at -1.905 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 7 smd rect (at -0.635 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(IC1-Pad7)"))
    (pad 6 smd rect (at 0.635 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(IC1-Pad6)"))
    (pad 5 smd rect (at 1.905 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(IC1-Pad5)"))
    (pad 4 smd rect (at 1.905 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0.635 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(IC1-Pad3)"))
    (pad 2 smd rect (at -0.635 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(IC1-Pad2)"))
    (pad 1 smd rect (at -1.905 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(IC1-Pad1)"))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connect:GS2 (layer F.Cu) (tedit 0) (tstamp 57BE9758)
    (at 169.964001 107.125239)
    (descr "Pontet Goute de soudure")
    (path /57BD62A1)
    (attr virtual)
    (fp_text reference JP1 (at 1.778 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Jumper_NC_Small (at 1.524 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.889 -1.27) (end -0.889 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.889 1.27) (end 0.889 -1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.889 1.27) (end -0.889 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.889 -1.27) (end 0.889 -1.27) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at 0 -0.635) (size 1.27 0.9652) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 0 0.635) (size 1.27 0.9652) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )

  (module Connect:GS3 (layer F.Cu) (tedit 0) (tstamp 57BE975F)
    (at 169.874001 127.214762)
    (descr "Pontet Goute de soudure")
    (path /57BD8FF3)
    (attr virtual)
    (fp_text reference JP2 (at 1.524 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value JUMPER3 (at 1.524 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.889 -1.905) (end -0.889 1.905) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.889 1.905) (end 0.889 1.905) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.889 1.905) (end 0.889 -1.905) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.889 -1.905) (end 0.889 -1.905) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at 0 -1.27) (size 1.27 0.9652) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(IC1-Pad3)"))
    (pad 2 smd rect (at 0 0) (size 1.27 0.9652) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(JP2-Pad2)"))
    (pad 3 smd rect (at 0 1.27) (size 1.27 0.9652) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(IC1-Pad1)"))
  )

  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 54EA090C) (tstamp 57BE9765)
    (at 163.683333 122.455)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /57BD7DBE)
    (fp_text reference P1 (at 0 -5.1) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X02 (at 0 -3.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.27 1.27) (end 1.27 3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.75 -1.75) (end -1.75 4.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 4.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 4.3) (end 1.75 4.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 1.27) (end -1.27 3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 3.81) (end 1.27 3.81) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 /V_BAT))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Connect:USB_Mini-B (layer F.Cu) (tedit 5543E571) (tstamp 57BE9774)
    (at 163.725001 108.4043)
    (descr "USB Mini-B 5-pin SMD connector")
    (tags "USB USB_B USB_Mini connector")
    (path /57BD722D)
    (attr smd)
    (fp_text reference P2 (at 0 6.90118) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value USB_OTG (at 0 -7.0993) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -4.85 -5.7) (end 4.85 -5.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.85 -5.7) (end 4.85 5.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.85 5.7) (end -4.85 5.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.85 5.7) (end -4.85 -5.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.59918 -3.85064) (end -3.59918 3.85064) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.59994 -3.85064) (end -4.59994 3.85064) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.59994 3.85064) (end 4.59994 3.85064) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.59994 3.85064) (end 4.59994 -3.85064) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.59994 -3.85064) (end -4.59994 -3.85064) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at 3.44932 -1.6002) (size 2.30124 0.50038) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at 3.44932 -0.8001) (size 2.30124 0.50038) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D3-Pad2)"))
    (pad 3 smd rect (at 3.44932 0) (size 2.30124 0.50038) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (pad 4 smd rect (at 3.44932 0.8001) (size 2.30124 0.50038) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(P2-Pad4)"))
    (pad 5 smd rect (at 3.44932 1.6002) (size 2.30124 0.50038) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 3.35026 -4.45008) (size 2.49936 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(P2-Pad6)"))
    (pad 6 smd rect (at -2.14884 -4.45008) (size 2.49936 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(P2-Pad6)"))
    (pad 6 smd rect (at 3.35026 4.45008) (size 2.49936 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(P2-Pad6)"))
    (pad 6 smd rect (at -2.14884 4.45008) (size 2.49936 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(P2-Pad6)"))
    (pad "" np_thru_hole circle (at 0.8509 -2.19964) (size 0.89916 0.89916) (drill 0.89916) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0.8509 2.19964) (size 0.89916 0.89916) (drill 0.89916) (layers *.Cu *.Mask F.SilkS))
  )

  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 54EA090C) (tstamp 57BE977A)
    (at 177.843333 106.405)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /57BD9D74)
    (fp_text reference P3 (at 0 -5.1) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X02 (at 0 -3.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.27 1.27) (end 1.27 3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.75 -1.75) (end -1.75 4.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 4.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 4.3) (end 1.75 4.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 1.27) (end -1.27 3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 3.81) (end 1.27 3.81) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x07 (layer F.Cu) (tedit 0) (tstamp 57BE9785)
    (at 153.623333 106.405)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /57BD8C98)
    (fp_text reference P4 (at 0 -5.1) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X07 (at 0 -3.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.75 -1.75) (end -1.75 17) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 17) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 17) (end 1.75 17) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.27 1.27) (end 1.27 16.51) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 16.51) (end -1.27 16.51) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 16.51) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(IC1-Pad5)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(IC1-Pad6)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(IC1-Pad7)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(IC1-Pad2)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(IC1-Pad3)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(IC1-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x07.wrl
      (at (xyz 0 -0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB) (tstamp 57BE978B)
    (at 193.945001 108.955)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (path /57BD61E2)
    (attr smd)
    (fp_text reference R1 (at 0 -2.1) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1K5 (at 0 2.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.6 -1) (end 1.6 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.6 1) (end 1.6 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.6 -1) (end -1.6 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.6 -1) (end 1.6 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.6 0.875) (end -0.6 0.875) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.6 -0.875) (end 0.6 -0.875) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D3-Pad2)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB) (tstamp 57BE9791)
    (at 174.295001 126.685)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (path /57BD5D42)
    (attr smd)
    (fp_text reference R2 (at 0 -2.1) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1K5 (at 0 2.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.6 -1) (end 1.6 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.6 1) (end 1.6 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.6 -1) (end -1.6 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.6 -1) (end 1.6 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.6 0.875) (end -0.6 0.875) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.6 -0.875) (end 0.6 -0.875) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D4-Pad2)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB) (tstamp 57BE9797)
    (at 178.595001 124.595)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (path /57BD9382)
    (attr smd)
    (fp_text reference R3 (at 0 -2.1) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 68R (at 0 2.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.6 -1) (end 1.6 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.6 1) (end 1.6 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.6 -1) (end -1.6 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.6 -1) (end 1.6 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.6 0.875) (end -0.6 0.875) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.6 -0.875) (end 0.6 -0.875) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(IC1-Pad2)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D3-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB) (tstamp 57BE979D)
    (at 201.005001 103.405)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (path /57BD93CB)
    (attr smd)
    (fp_text reference R4 (at 0 -2.1) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 68R (at 0 2.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.6 -1) (end 1.6 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.6 1) (end 1.6 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.6 -1) (end -1.6 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.6 -1) (end 1.6 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.6 0.875) (end -0.6 0.875) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.6 -0.875) (end 0.6 -0.875) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(JP2-Pad2)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Buttons_Switches_SMD:SW_SPST_EVQPE1 (layer F.Cu) (tedit 5788B2FA) (tstamp 57BE97A3)
    (at 187.045001 111.895)
    (descr "Light Touch Switch")
    (path /57BD99EB)
    (attr smd)
    (fp_text reference SW1 (at -0.9 -2.7) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_PUSH (at 0 3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.95 -2) (end 3.95 -2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.95 -2) (end 3.95 2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.95 2) (end -3.95 2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.95 2) (end -3.95 -2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3 -1.75) (end 3 -1.1) (layer F.SilkS) (width 0.15))
    (fp_line (start 3 1.75) (end 3 1.1) (layer F.SilkS) (width 0.15))
    (fp_line (start -3 1.1) (end -3 1.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -3 -1.75) (end -3 -1.1) (layer F.SilkS) (width 0.15))
    (fp_line (start 3 -1.75) (end -3 -1.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -3 1.75) (end 3 1.75) (layer F.SilkS) (width 0.15))
    (pad 2 smd rect (at 2.7 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.7 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(IC1-Pad1)"))
  )

  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 0) (tstamp 57BE97AB)
    (at 172.785714 118.767001)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (path /57BDA9DC)
    (attr smd)
    (fp_text reference U1 (at 0 -0.762) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value AP111750 (at 0 0.762) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.556 1.524) (end -3.556 4.572) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.556 4.572) (end 3.556 4.572) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.556 4.572) (end 3.556 1.524) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.556 -1.524) (end -3.556 -2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.556 -2.286) (end -2.032 -4.572) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.032 -4.572) (end 2.032 -4.572) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.032 -4.572) (end 3.556 -2.286) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.556 -2.286) (end 3.556 -1.524) (layer F.SilkS) (width 0.15))
    (pad 4 smd rect (at 0 -3.302) (size 3.6576 2.032) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 3 smd rect (at 2.286 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 1 /V_BAT))
    (pad 1 smd rect (at -2.286 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )

)
