(footprint "ETH-MAGJACK" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr through_hole)
  (fp_text reference "ETH-MAGJACK" (at -3.175 -12.065) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 8b8b2473-1469-49d2-af1b-b0988ed44931)
  )
  (fp_text value "VAL**" (at -6.35 -13.97) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 589e0675-cd31-4e9b-99f6-dc712de15e26)
  )
  (fp_text user "Board edge" (at -4 8.6 unlocked) (layer "Cmts.User")
      (effects (font (size 1 1) (thickness 0.15)) (justify left bottom))
    (tstamp 47b4f11d-6f03-47a3-a182-e55b9e8236e7)
  )
  (fp_line (start -8.255 -11.43) (end -8.255 -5)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp ab06046d-f3f3-4217-b8d0-714a1127c921))
  (fp_line (start -8.255 -1) (end -8.255 6.9)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp dcfbd880-0e1b-482d-a297-0efb33ca3a04))
  (fp_line (start 8.255 -11.43) (end -8.255 -11.43)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 7cfbcac4-d4b5-4b72-a820-68d6c6b5fa3b))
  (fp_line (start 8.255 -5) (end 8.255 -11.43)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp e51668fd-730b-4055-b071-6db48ce2fd3e))
  (fp_line (start 8.255 6.9) (end 8.255 -1)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 3d313d3f-191e-47fd-b3bf-4c7697ede91d))
  (fp_line (start -9.4 6.9) (end 9.4 6.9)
    (stroke (width 0.12) (type default)) (layer "Cmts.User") (tstamp 4ee227f9-8c8f-4b4c-a78a-caaa7997b7a2))
  (fp_line (start -9.4 -3.8) (end -8.4 -4.6)
    (stroke (width 0.12) (type default)) (layer "B.CrtYd") (tstamp 36afe1a8-3f12-45f9-82d4-39029098c4f5))
  (fp_line (start -9.4 -2.4) (end -9.4 -3.8)
    (stroke (width 0.12) (type default)) (layer "B.CrtYd") (tstamp 7c1e902d-59b0-4de7-a993-ad5ea1ffdc1a))
  (fp_line (start -8.4 -4.6) (end -7 -4.6)
    (stroke (width 0.12) (type default)) (layer "B.CrtYd") (tstamp 9b9fa2cd-1d69-4306-a42b-d0574d562950))
  (fp_line (start -8.4 -1.4) (end -9.4 -2.4)
    (stroke (width 0.12) (type default)) (layer "B.CrtYd") (tstamp 31ffcf34-9424-48f2-b0ac-f448b8b47560))
  (fp_line (start -8.4 5.4) (end -8.4 -1.4)
    (stroke (width 0.12) (type default)) (layer "B.CrtYd") (tstamp 4fa0f412-0a6f-471c-8f62-ea72a2cded73))
  (fp_line (start -7 -4.6) (end -4.2 -1.8)
    (stroke (width 0.12) (type default)) (layer "B.CrtYd") (tstamp 7f78f41d-0788-4c14-bcc7-cdc2a0ef44fd))
  (fp_line (start -5.8 -7.6) (end -4 -10)
    (stroke (width 0.12) (type default)) (layer "B.CrtYd") (tstamp 36495345-9501-498a-b9a9-eea5f3e1422d))
  (fp_line (start -5.8 -6) (end -5.8 -7.6)
    (stroke (width 0.12) (type default)) (layer "B.CrtYd") (tstamp a559eaf1-391c-47a2-bf5f-596926c9ac06))
  (fp_line (start -5.4 2.6) (end -5.4 5.4)
    (stroke (width 0.12) (type default)) (layer "B.CrtYd") (tstamp e2b87989-c7e5-4cc5-adfb-808f7849b1ac))
  (fp_line (start -5.4 5.4) (end -8.4 5.4)
    (stroke (width 0.12) (type default)) (layer "B.CrtYd") (tstamp 9cd24f7c-b486-40e8-b88c-51e942a336d7))
  (fp_line (start -5.2 -5.2) (end -5.8 -6)
    (stroke (width 0.12) (type default)) (layer "B.CrtYd") (tstamp 17397842-e593-4a97-981e-996eaad9ca95))
  (fp_line (start -4.2 -1.8) (end -3.4 -1)
    (stroke (width 0.12) (type default)) (layer "B.CrtYd") (tstamp 9c380f47-7fc5-494e-80a4-825fe4eaa742))
  (fp_line (start -4 -10) (end 5.4 -10)
    (stroke (width 0.12) (type default)) (layer "B.CrtYd") (tstamp 3ef67efe-b3f0-4f01-be50-5f85285170f1))
  (fp_line (start -3.4 -1) (end -3.4 1.2)
    (stroke (width 0.12) (type default)) (layer "B.CrtYd") (tstamp 83d752b8-c0d4-4dd4-bd28-1c262460289d))
  (fp_line (start -3.4 1.2) (end -5.4 2.6)
    (stroke (width 0.12) (type default)) (layer "B.CrtYd") (tstamp bd1bd05c-1bdc-41b7-ae96-d0a8b2df8f59))
  (fp_line (start 3.6 -1.2) (end 7.2 -4.8)
    (stroke (width 0.12) (type default)) (layer "B.CrtYd") (tstamp c87355dd-41e1-4359-b027-0094737275b5))
  (fp_line (start 3.6 1.2) (end 3.6 -1.2)
    (stroke (width 0.12) (type default)) (layer "B.CrtYd") (tstamp 3bd40b3c-faf0-46cb-8e7f-0809142a5c9a))
  (fp_line (start 3.8 -5.2) (end -5.2 -5.2)
    (stroke (width 0.12) (type default)) (layer "B.CrtYd") (tstamp f4bd2b38-1495-43d8-bebc-edf9b7188c8e))
  (fp_line (start 5.4 -10) (end 5.4 -7.6)
    (stroke (width 0.12) (type default)) (layer "B.CrtYd") (tstamp 93f78e28-4cae-4f4c-bd7f-883c0ff18e53))
  (fp_line (start 5.4 -7.6) (end 3.8 -5.2)
    (stroke (width 0.12) (type default)) (layer "B.CrtYd") (tstamp 9400675b-a9dd-4d53-b4d0-6319a70c9248))
  (fp_line (start 5.4 2.6) (end 3.6 1.2)
    (stroke (width 0.12) (type default)) (layer "B.CrtYd") (tstamp ea917281-f341-4e6a-95e5-e050c5d85f7c))
  (fp_line (start 5.4 5.6) (end 5.4 2.6)
    (stroke (width 0.12) (type default)) (layer "B.CrtYd") (tstamp c97fa274-e578-418c-aa8a-25cf9e7de978))
  (fp_line (start 7.2 -4.8) (end 8.4 -4.8)
    (stroke (width 0.12) (type default)) (layer "B.CrtYd") (tstamp 721d901d-c8b6-495a-94ed-14ccde20a3bc))
  (fp_line (start 8.4 -4.8) (end 9.4 -3.8)
    (stroke (width 0.12) (type default)) (layer "B.CrtYd") (tstamp 75e9b1fd-65e3-4360-9a0b-652d42d96f10))
  (fp_line (start 8.4 -1.4) (end 8.4 5.6)
    (stroke (width 0.12) (type default)) (layer "B.CrtYd") (tstamp d3bbc993-6c89-46c6-b523-652ad52c3e4d))
  (fp_line (start 8.4 5.6) (end 5.4 5.6)
    (stroke (width 0.12) (type default)) (layer "B.CrtYd") (tstamp 28859df1-0ccf-4077-84db-41e78fa3f694))
  (fp_line (start 9.4 -3.8) (end 9.4 -2.4)
    (stroke (width 0.12) (type default)) (layer "B.CrtYd") (tstamp 1a9e99a6-ffc6-4967-9e67-34bb03aabd18))
  (fp_line (start 9.4 -2.4) (end 8.4 -1.4)
    (stroke (width 0.12) (type default)) (layer "B.CrtYd") (tstamp 78f6c0b8-52c0-4d95-82d8-641ef4ae5dc3))
  (fp_line (start -9.4 -3.8) (end -8.4 -4.6)
    (stroke (width 0.12) (type default)) (layer "F.CrtYd") (tstamp 70aa9aa8-83a5-467a-a7d8-45ecb47f6b27))
  (fp_line (start -9.4 -2.4) (end -9.4 -3.8)
    (stroke (width 0.12) (type default)) (layer "F.CrtYd") (tstamp 2405d3b0-8ad4-4c39-8f71-fec7447d31fa))
  (fp_line (start -8.4 -11.6) (end 8.4 -11.6)
    (stroke (width 0.12) (type default)) (layer "F.CrtYd") (tstamp 21e5f533-1a5d-4471-856b-1c0da5e792a6))
  (fp_line (start -8.4 -4.6) (end -8.4 -11.6)
    (stroke (width 0.12) (type default)) (layer "F.CrtYd") (tstamp 233a5dc0-67fa-42fb-b165-617b91ff0159))
  (fp_line (start -8.4 -1.4) (end -9.4 -2.4)
    (stroke (width 0.12) (type default)) (layer "F.CrtYd") (tstamp 6b72943b-79d2-4fe3-bad5-7c1f9b258f4a))
  (fp_line (start -8.4 10.4) (end -8.4 -1.4)
    (stroke (width 0.12) (type default)) (layer "F.CrtYd") (tstamp 3fafa363-7fa5-4715-b233-d4ba9ec966c1))
  (fp_line (start 8.4 -11.6) (end 8.4 -4.8)
    (stroke (width 0.12) (type default)) (layer "F.CrtYd") (tstamp d0413213-4590-45a5-b811-5b83e7cfcd6e))
  (fp_line (start 8.4 -4.8) (end 9.4 -3.8)
    (stroke (width 0.12) (type default)) (layer "F.CrtYd") (tstamp 1e676530-7dba-40e9-8610-00b847a2369d))
  (fp_line (start 8.4 -1.4) (end 8.4 10.4)
    (stroke (width 0.12) (type default)) (layer "F.CrtYd") (tstamp b352188e-57f5-4f78-b4cb-73f00cb048e6))
  (fp_line (start 8.4 10.4) (end -8.4 10.4)
    (stroke (width 0.12) (type default)) (layer "F.CrtYd") (tstamp 200adf78-eaf8-4670-9d8e-a91ade4a6440))
  (fp_line (start 9.4 -3.8) (end 9.4 -2.4)
    (stroke (width 0.12) (type default)) (layer "F.CrtYd") (tstamp 2109b463-ab2b-4a3f-b8c4-40f8a5058977))
  (fp_line (start 9.4 -2.4) (end 8.4 -1.4)
    (stroke (width 0.12) (type default)) (layer "F.CrtYd") (tstamp d6cad863-639f-4067-bf1c-5293d7dbec67))
  (pad "" np_thru_hole circle (at -5.715 0) (size 3.2 3.2) (drill 3.2) (layers "*.Mask") (tstamp 57512c43-99a9-44ed-a503-b23cc1348550))
  (pad "" np_thru_hole circle (at 5.715 0) (size 3.2 3.2) (drill 3.2) (layers "*.Mask") (tstamp 372a0054-15f4-4052-90b2-11a344767066))
  (pad "1" thru_hole circle (at -4.445 -6.35) (size 1.6 1.6) (drill 0.9) (layers "*.Cu" "*.Mask") (tstamp bbf07e5d-c58a-4a1f-9097-06fd891ee91b))
  (pad "2" thru_hole circle (at -3.175 -8.89) (size 1.6 1.6) (drill 0.9) (layers "*.Cu" "*.Mask") (tstamp 5d9fe8fe-f7dd-438d-9ea9-eaea1436334b))
  (pad "3" thru_hole circle (at -1.905 -6.35) (size 1.6 1.6) (drill 0.9) (layers "*.Cu" "*.Mask") (tstamp 96ad49a6-4eee-4923-84a9-71c96df4bb88))
  (pad "4" thru_hole circle (at -0.635 -8.89) (size 1.6 1.6) (drill 0.9) (layers "*.Cu" "*.Mask") (tstamp cb3b85e1-6012-4a1a-83ba-d93c08267daf))
  (pad "5" thru_hole circle (at 0.635 -6.35) (size 1.6 1.6) (drill 0.9) (layers "*.Cu" "*.Mask") (tstamp 3952cdb2-163b-414b-9233-66e3bd276f11))
  (pad "6" thru_hole circle (at 1.905 -8.89) (size 1.6 1.6) (drill 0.9) (layers "*.Cu" "*.Mask") (tstamp a8cf9c7b-e217-40c7-a6a0-712dc21b9197))
  (pad "7" thru_hole circle (at 3.175 -6.35) (size 1.6 1.6) (drill 0.9) (layers "*.Cu" "*.Mask") (tstamp 00ed9840-8180-4b0b-a499-96add2f44a4e))
  (pad "8" thru_hole circle (at 4.445 -8.89) (size 1.6 1.6) (drill 0.9) (layers "*.Cu" "*.Mask") (tstamp e666ac14-59d9-4977-976a-0a4ec8a450e5))
  (pad "9" thru_hole circle (at -7.747 -3.048) (size 2.2 2.2) (drill 1.6) (layers "*.Cu" "*.Mask") (tstamp 386e1020-665b-4176-b6d6-d7d3b235bed9))
  (pad "10" thru_hole circle (at 7.747 -3.048) (size 2.2 2.2) (drill 1.6) (layers "*.Cu" "*.Mask") (tstamp 8ccda25d-4268-40cb-a7da-6dd507e2d995))
  (pad "11" thru_hole circle (at -6.7818 2.54) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 5bc60c4c-a98e-4e87-bb69-a99548b703a1))
  (pad "12" thru_hole circle (at -6.7818 4.572) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask") (tstamp c5dbe86e-3f5e-46ca-9c14-5b219753da9c))
  (pad "13" thru_hole circle (at 6.7818 2.54) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 6c1cc590-93f8-499b-8d03-a8e9228613e1))
  (pad "14" thru_hole circle (at 6.7818 4.572) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 859a41f0-761f-4adb-bd67-34bf3ff11bd0))
)
