(export (version D)
  (design
    (source /home/yair/dev/at-tami/kicad/attami.sch)
    (date "Thu 25 Aug 2016 09:41:58 AM IDT")
    (tool "Eeschema 4.0.3-stable")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title ATtami)
        (company telavivmakers.org)
        (rev)
        (date 2016-08-24)
        (source attami.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref IC1)
      (value ATTINY85-S)
      (footprint SMD_Packages:SOIC-8-N)
      (libsource (lib attami-cache) (part ATTINY85-S))
      (sheetpath (names /) (tstamps /))
      (tstamp 57BD5CB6))
    (comp (ref R2)
      (value 1K5)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib attami-cache) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 57BD5D42))
    (comp (ref R1)
      (value 1K5)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib attami-cache) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 57BD61E2))
    (comp (ref D4)
      (value "red LED")
      (footprint LEDs:LED_0805)
      (libsource (lib attami-cache) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 57BD624D))
    (comp (ref JP1)
      (value Jumper_NC_Small)
      (footprint Connect:GS2)
      (libsource (lib attami-cache) (part Jumper_NC_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 57BD62A1))
    (comp (ref C1)
      (value 1uf)
      (footprint Capacitors_SMD:C_0805)
      (libsource (lib attami-cache) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 57BD6F3C))
    (comp (ref C2)
      (value 2.2uf)
      (footprint Capacitors_SMD:C_0805)
      (libsource (lib attami-cache) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 57BD6FAC))
    (comp (ref P2)
      (value USB_OTG)
      (footprint Connect:USB_Mini-B)
      (libsource (lib attami-cache) (part USB_OTG))
      (sheetpath (names /) (tstamps /))
      (tstamp 57BD722D))
    (comp (ref D2)
      (value D_Schottky)
      (footprint Diodes_SMD:SOD-323)
      (libsource (lib attami-cache) (part D_Schottky))
      (sheetpath (names /) (tstamps /))
      (tstamp 57BD74D6))
    (comp (ref D1)
      (value "blue LED")
      (footprint LEDs:LED_0805)
      (libsource (lib attami-cache) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 57BD75CA))
    (comp (ref P1)
      (value CONN_01X02)
      (footprint Pin_Headers:Pin_Header_Straight_1x02)
      (libsource (lib attami-cache) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 57BD7DBE))
    (comp (ref D3)
      (value "blue LED")
      (footprint LEDs:LED_0805)
      (libsource (lib attami-cache) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 57BD80DC))
    (comp (ref P4)
      (value CONN_01X07)
      (footprint Pin_Headers:Pin_Header_Straight_1x07)
      (libsource (lib attami-cache) (part CONN_01X07))
      (sheetpath (names /) (tstamps /))
      (tstamp 57BD8C98))
    (comp (ref JP2)
      (value JUMPER3)
      (footprint Connect:GS3)
      (libsource (lib attami-cache) (part JUMPER3))
      (sheetpath (names /) (tstamps /))
      (tstamp 57BD8FF3))
    (comp (ref R3)
      (value 68R)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib attami-cache) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 57BD9382))
    (comp (ref R4)
      (value 68R)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib attami-cache) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 57BD93CB))
    (comp (ref SW1)
      (value SW_PUSH)
      (footprint Buttons_Switches_SMD:SW_SPST_EVQPE1)
      (libsource (lib attami-cache) (part SW_PUSH))
      (sheetpath (names /) (tstamps /))
      (tstamp 57BD99EB))
    (comp (ref P3)
      (value CONN_01X02)
      (footprint Pin_Headers:Pin_Header_Straight_1x02)
      (libsource (lib attami-cache) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 57BD9D74))
    (comp (ref U1)
      (value AP111750)
      (footprint TO_SOT_Packages_SMD:SOT-223)
      (libsource (lib attami-cache) (part AP111750))
      (sheetpath (names /) (tstamps /))
      (tstamp 57BDA9DC)))
  (libparts
    (libpart (lib attami-cache) (part AP1117)
      (aliases
        (alias AP111715)
        (alias AP111718)
        (alias AP111725)
        (alias AP111733)
        (alias AP111750))
      (footprints
        (fp SOT-223*))
      (fields
        (field (name Reference) U)
        (field (name Value) AP1117)
        (field (name Footprint) TO_SOT_Packages_SMD:SOT-223))
      (pins
        (pin (num 1) (name GND/ADJ) (type power_in))
        (pin (num 2) (name VO) (type power_out))
        (pin (num 3) (name VI) (type power_in))
        (pin (num 4) (name VO) (type power_out))))
    (libpart (lib attami-cache) (part ATTINY25-S)
      (aliases
        (alias ATTINY45-S)
        (alias ATTINY85-S))
      (fields
        (field (name Reference) IC)
        (field (name Value) ATTINY25-S)
        (field (name Footprint) SO8-200))
      (pins
        (pin (num 1) (name "PB5(~RESET~/dW/ADC0/PCINT5)") (type BiDi))
        (pin (num 2) (name "PB3(XTAL1/CLKI/OC1B/ADC3/PCINT3)") (type BiDi))
        (pin (num 3) (name "PB4(XTAL2/CLKO/OC1B/ADC2/PCINT4)") (type BiDi))
        (pin (num 4) (name GND) (type power_in))
        (pin (num 5) (name "PB0(MOSI/DI/SDA/AIN0/OC0A/OC1A/AREF/PCINT0)") (type BiDi))
        (pin (num 6) (name "PB1(MISO/DO/AIN1/OC0B/OC1A/PCINT1)") (type BiDi))
        (pin (num 7) (name "PB2(SCK/USCK/SCL/T0/INT0/ADC1/PCINT2)") (type BiDi))
        (pin (num 8) (name VCC) (type power_in))))
    (libpart (lib attami-cache) (part C)
      (footprints
        (fp C?)
        (fp C_????_*)
        (fp C_????)
        (fp SMD*_c)
        (fp Capacitor*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib attami-cache) (part CONN_01X02)
      (footprints
        (fp Pin_Header_Straight_1X02)
        (fp Pin_Header_Angled_1X02)
        (fp Socket_Strip_Straight_1X02)
        (fp Socket_Strip_Angled_1X02))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X02))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))))
    (libpart (lib attami-cache) (part CONN_01X07)
      (footprints
        (fp Pin_Header_Straight_1X07)
        (fp Pin_Header_Angled_1X07)
        (fp Socket_Strip_Straight_1X07)
        (fp Socket_Strip_Angled_1X07))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X07))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))))
    (libpart (lib attami-cache) (part D_Schottky)
      (footprints
        (fp D-Pak_TO252AA)
        (fp Diode_*)
        (fp *SingleDiode)
        (fp *SingleDiode*)
        (fp *_Diode_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D_Schottky))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib attami-cache) (part JUMPER3)
      (fields
        (field (name Reference) JP)
        (field (name Value) JUMPER3))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))))
    (libpart (lib attami-cache) (part Jumper_NC_Small)
      (fields
        (field (name Reference) JP)
        (field (name Value) Jumper_NC_Small))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib attami-cache) (part LED)
      (footprints
        (fp LED-*)
        (fp LED_*))
      (fields
        (field (name Reference) D)
        (field (name Value) LED))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib attami-cache) (part R)
      (footprints
        (fp R_*)
        (fp Resistor_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib attami-cache) (part SW_PUSH)
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_PUSH))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib attami-cache) (part USB_OTG)
      (footprints
        (fp USB*))
      (fields
        (field (name Reference) P)
        (field (name Value) USB_OTG))
      (pins
        (pin (num 1) (name VCC) (type power_out))
        (pin (num 2) (name D-) (type passive))
        (pin (num 3) (name D+) (type passive))
        (pin (num 4) (name ID) (type power_in))
        (pin (num 5) (name GND) (type power_in))
        (pin (num 6) (name shield) (type passive)))))
  (libraries
    (library (logical attami-cache)
      (uri /home/yair/dev/at-tami/kicad/attami-cache.lib)))
  (nets
    (net (code 1) (name "Net-(D2-Pad2)")
      (node (ref P2) (pin 1))
      (node (ref D2) (pin 2)))
    (net (code 2) (name "Net-(D3-Pad2)")
      (node (ref D3) (pin 2))
      (node (ref P2) (pin 2))
      (node (ref R3) (pin 2))
      (node (ref R1) (pin 1)))
    (net (code 3) (name GND)
      (node (ref SW1) (pin 2))
      (node (ref P3) (pin 1))
      (node (ref C1) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref P2) (pin 5))
      (node (ref JP1) (pin 2))
      (node (ref D1) (pin 1))
      (node (ref P1) (pin 1))
      (node (ref IC1) (pin 4))
      (node (ref U1) (pin 1))
      (node (ref D3) (pin 1))
      (node (ref P4) (pin 1)))
    (net (code 4) (name "Net-(IC1-Pad2)")
      (node (ref IC1) (pin 2))
      (node (ref P4) (pin 5))
      (node (ref R3) (pin 1)))
    (net (code 5) (name "Net-(D4-Pad2)")
      (node (ref D4) (pin 2))
      (node (ref R2) (pin 1)))
    (net (code 6) (name "Net-(JP2-Pad2)")
      (node (ref JP2) (pin 2))
      (node (ref R4) (pin 1)))
    (net (code 7) (name "Net-(IC1-Pad3)")
      (node (ref P4) (pin 6))
      (node (ref JP2) (pin 1))
      (node (ref IC1) (pin 3)))
    (net (code 8) (name "Net-(IC1-Pad1)")
      (node (ref P4) (pin 7))
      (node (ref IC1) (pin 1))
      (node (ref SW1) (pin 1))
      (node (ref JP2) (pin 3)))
    (net (code 9) (name "Net-(IC1-Pad5)")
      (node (ref IC1) (pin 5))
      (node (ref P4) (pin 2)))
    (net (code 10) (name "Net-(D4-Pad1)")
      (node (ref JP1) (pin 1))
      (node (ref D4) (pin 1)))
    (net (code 11) (name "Net-(IC1-Pad6)")
      (node (ref P4) (pin 3))
      (node (ref IC1) (pin 6)))
    (net (code 12) (name "Net-(IC1-Pad7)")
      (node (ref P4) (pin 4))
      (node (ref IC1) (pin 7)))
    (net (code 13) (name "Net-(P2-Pad4)")
      (node (ref P2) (pin 4)))
    (net (code 14) (name "Net-(P2-Pad6)")
      (node (ref P2) (pin 6)))
    (net (code 15) (name "Net-(D1-Pad2)")
      (node (ref D1) (pin 2))
      (node (ref P2) (pin 3))
      (node (ref R4) (pin 2)))
    (net (code 16) (name VCC)
      (node (ref U1) (pin 2))
      (node (ref R1) (pin 2))
      (node (ref U1) (pin 4))
      (node (ref R2) (pin 2))
      (node (ref IC1) (pin 8))
      (node (ref D2) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref P3) (pin 2)))
    (net (code 17) (name /V_BAT)
      (node (ref U1) (pin 3))
      (node (ref C1) (pin 1))
      (node (ref P1) (pin 2)))))