<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="22.829840625" y2="0" width="0" layer="20"/>
<wire x1="22.829840625" y1="0" x2="22.829840625" y2="22.8602" width="0" layer="20"/>
<wire x1="22.829840625" y1="22.8602" x2="0" y2="22.8602" width="0" layer="20"/>
<wire x1="0" y1="22.8602" x2="0" y2="0" width="0" layer="20"/>
<text>VCC</text>
<text>PB2</text>
<text>PB1</text>
<text>PB0</text>
<text>PB3</text>
<text>PB4</text>
<text>PB5</text>
<text>BAT</text>
<text>J2</text>
<text>PB2</text>
<text>PB1</text>
<text>PB0</text>
<text>PB3</text>
<text>PB4</text>
<text>PB5</text>
<text>BAT</text>
<text>VCC</text>
<text>+</text>
<text>to hide the silkscreen:
disable layers: tNames, bNames, tPlace, bPlace</text>
<text>more at   github.com/telavivmakers/at-tami</text>
<text>V 0.00</text>
</plain>
<libraries>
<library name="ohw-logo">
<packages>
<package name="OSHW_6X150_NOTEXT">
</package>
</packages>
</library>
<library name="ATtami">
<packages>
<package name="1X02_ROUND">
</package>
<package name="1X07_ROUND">
</package>
<package name="MOUNTINGHOLE_2.0_PLATED">
</package>
</packages>
</library>
<library name="SparkFunNew">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO16">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
<package name="RESONATOR-SMD">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="ATtami" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0"/>
<element name="U$2" library="ATtami" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0"/>
<element name="J2" library="ATtami" package="1X02_ROUND" value="">
<attribute name="NAME"/>
</element>
<element name="J3" library="ATtami" package="1X02_ROUND" value="">
<attribute name="NAME"/>
</element>
<element name="J1" library="ATtami" package="1X07_ROUND" value="">
<attribute name="VALUE"/>
</element>
<element name="U$3" library="ohw-logo" package="OSHW_6X150_NOTEXT" value=""/>
<element name="CH340" library="SparkFunNew" package="SO16" value="CH340G"/>
<element name="C2" library="adafruit" package="C0603" value="0.1u"/>
<element name="C3" library="adafruit" package="C0603" value="0.1u"/>
<element name="X2" library="SparkFunNew" package="RESONATOR-SMD" value="12MHz"/>
</elements>
<signals>
<signal name="GND">
<contactref element="J3" pad="2"/>
<contactref element="J2" pad="2"/>
<contactref element="J1" pad="1"/>
<contactref element="CH340" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="X2" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="J3" pad="1"/>
<contactref element="CH340" pad="16"/>
<contactref element="C2" pad="1"/>
<contactref element="CH340" pad="4"/>
</signal>
<signal name="N$2">
</signal>
<signal name="N$9">
</signal>
<signal name="N$12">
</signal>
<signal name="N$3">
<contactref element="J2" pad="1"/>
</signal>
<signal name="PB0">
<contactref element="J1" pad="2"/>
<contactref element="CH340" pad="6"/>
</signal>
<signal name="PB1">
<contactref element="J1" pad="3"/>
<contactref element="CH340" pad="5"/>
</signal>
<signal name="PB2">
<contactref element="J1" pad="4"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="PB3">
<contactref element="J1" pad="5"/>
</signal>
<signal name="PB4">
<contactref element="J1" pad="6"/>
</signal>
<signal name="PB5">
<contactref element="J1" pad="7"/>
</signal>
<signal name="RXD">
<contactref element="CH340" pad="2"/>
</signal>
<signal name="TXD">
<contactref element="CH340" pad="3"/>
</signal>
<signal name="RST">
<contactref element="CH340" pad="14"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="CH340" pad="7"/>
<contactref element="X2" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="X2" pad="3"/>
<contactref element="CH340" pad="8"/>
</signal>
<signal name="N$1">
</signal>
</signals>
</board>
</drawing>
</eagle>
